**Q1:**

**Konrad Dittrich, Simon Spång**

A stabilizable system will reach the desired state for a control input . If a system is not stabilizable no minimum of the LQR problem can be found since the state cost will increase continuously.

A reachability test could be performed since a reachable system is also stabilizable. Reachability is a necessary condition for stabilizability. Therefore, the full rank of the controllability Matrix or the PBH test is to be checked.

The PBH test for reachability is performed: A system (A, B) is unreachable if and only if there exists a left hand eigenvector with such that:

and .

The calculation delivers the following eigenvalues:

As a result, the system is reachable and since the reasoning above it’s also stabilizable.

**Q2:**

Figure 1 shows the original response without modification of Q or R.




Figure : Astrobee states over simulation time with no modified Q or R matrix

**R multiplied with 10:**

By multiplying the R matrix by factor 10 the control input is penalized stronger so that smaller control values are calculated. As a result, it the time to reach the desired states is increased since the focus is on low control input, see figure 2. The translational and rotational velocity is also lower.

Ein Bild, das Text, Reihe, Diagramm, Screenshot enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with R = 10

**Addition of Q[3:6] and Q[9:] with 100:**

By increasing the penalty on the translational velocities and rotational velocities by adding 100, the rise time for the position and attitude have been increased. The translational velocities and rotational velocities have also been decreased. The Astrobee doesn’t reach its desired positional state or attitude. See the plot in figure 3.

**Ein Bild, das Text, Reihe, Diagramm, Screenshot enthält.

Automatisch generierte Beschreibung**

Figure : Astrobee with Q[3:6] = 100 and Q[9:] = 100

**Addition of Q[0:3] and Q[6:9] with 100:**

By high penalization of position and attitude, these state are reach in short time, since its minimum is only found if these variables are reaching their desired state as fast as possible. This leads to an increase of the translational and rotational velocities. See figure 4.

Ein Bild, das Text, Reihe, Diagramm, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with 100 penalized position and attitude

**Addition of 100 to all elements of Q:**

By increasing all elements of Q with 100, the penalty of the controller becomes decreased, i.e. larger control actions is possible. As seen in figure 5 the rise time for the position and attitude is decreased and translational and rotational velocities are increased which is the result of a more aggressive controller.

En bild som visar text, linje, diagram, Parallell

Automatiskt genererad beskrivning

Figure - Astrobee with all Q elements increased with 100

**Q3:**

The requirements are met by the following weighting matrices:

For the weights of the Q-Matrix we found:

The following requirements are fulfilled, see also figure 5:

* Max distance to reference:
* Max speed:
* Max forces:

* Max torques:
* Max Euler angle deviations: (
* Overshoot

fullfilled

*Ein Bild, das Text, Reihe, Diagramm, parallel enthält.

Automatisch generierte Beschreibung*

Figure : Astrobee with multioptimized states and constraints

**Q4:**

The performance of the controller is influenced measurement noise now. The matrix is the input of this measurement noise for the Kalman filter. Small position deviations are detected, see Figure 6.

Ein Bild, das Text, Reihe, Diagramm, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with measurement noise: No huge deviations

To find out more about the influence of the measurement noise on the control, the measurement noise is increased from (-0.1, 0.1) to (-1, 1). It results in a highly disturbed position and velocity states that do not meet the requirements anymore. For example, the requirement of a maximum deviation of 2 cm on the position for the time after 12 sec does not hold anymore. Also the control effort is much higher because the system does not stabilize on one value and has to be controlled always to tend to the reference state.

Ein Bild, das Text, Diagramm, Reihe, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with high measurement noise of amount (-1,1): huge deviations in position and speed

**Q5:**

Now process noise is included to make the system more realistic. The matrix represents the process noise for the Kalman filter, see Figure 7.

Ein Bild, das Text, Diagramm, Reihe, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with measurement noise of given distribution of (-0.05, 0.05) and & factorized with 1

By increasing the measurement noise, the deviations get more severe, but the system still stays stable, see Figure 8.

Ein Bild, das Text, Diagramm, Reihe, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with estimated position, measurement noise of (-0.1, 0.1), process noise (-0.005, 0.005) and & factorized with 10

By adding high measurement noise (-1,1) and process noise (-0.005, 0.005) the performance of the system decreases more. The -position of the astrobee is for example deviating more than

Ein Bild, das Text, Diagramm, Reihe, parallel enthält.

Automatisch generierte Beschreibung

Figure : Astrobee with high measurement noise (-1,1) and process noise (-0.05, 0.05)